**RF Choke Information**

Plate Choke for 813 tube:

129 turns counter-clockwise, close-wound

3 – 3/8” long

Wound on 11/16” diameter ceramic or glass rod

>ham>chokes