The RCA Radiotron Designer's Handbook (4th ed., p. 1343), lists the RMA standard for chassis wiring colors as follows:

Black - grounds, grounded elements, and returns.

Brown - heaters or filaments, off ground

Red - power supply B+

Orange - screen grids

Yellow – cathodes

Green - control grids

Blue – plates

Violet - not used

Grey - A.C. power lines (this might need updating)

White - above or below ground returns, AVC, etc.