The RCA Radiotron Designer's Handbook (4th ed., p. 1343), lists the RMA standard for chassis wiring colors as follows:

Black - grounds, grounded elements, and returns.  
  
Brown - heaters or filaments, off ground  
  
Red - power supply B+  
  
Orange - screen grids  
  
Yellow – cathodes  
  
Green - control grids  
  
Blue – plates

Violet - not used  
  
Grey - A.C. power lines (this might need updating)  
  
White - above or below ground returns, AVC, etc.